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Shanghai Jianghuai Environmental Equipment Co.,LTD       

Address: No.2556,Gaoshi Road ,JiaDing District .shanghai City 

Tel.:+86 021 59970661 Fax: +86 021 59970661
Before the first use of equipment ,please read equipment operating .

When ordering replacement parts,pls kindly check the Parts manual that came with the machine. Before matching the accessories, please make sure your machine model and serial number.You can connect us by by telephone or mail.If you can and then do the following, you will be able to get the best results at the lowest cost:

● operating the machine carefully
● Pls maintenance the machine regularly according to the Maintenance Instructions of operating guide 
●Pls maintance with the same level of accessories or using the original accessories. 
Shanghai jianghuai environmental equipment CO.,LTD
Add:NO.2556, Gaoshi Road ,Jiading District , Shanghai City 
TEL.:+86-021-59970661      FAX:+86-021-59970661
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Precautions

This machine is suitable for industrial and commercial purposes, specifically for cleaning interior hard floors.

Please use the recommended scouring pads , brushes, and commercially floor cleaners which is applicable to this machine .
All operators must read, understand and observe the following safety precautions.
The following are explained for the safety alert symbol and "For security purposes" title:
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Warning: for warning serious injury or death risks or unsafe operation.
FOR SAFETY: To identify actions that must be followed when using the machine in order to guarantee safety.
Failure to comply with these warnings may result in: personal injury, electrocution, fire, or explosion.
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WARNING: Fire or explosion hazard
－Do not use flammable liquids; Do not operate the machine near or flammable liquids, gases or combustible dust workplace .
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This machine is not equipped with an explosion proof motor. If you use the machine in a place with flammable gas, liquid or flammable dust may be in start-up and during the operating of the electric motor will produce a spark, may cause a flash fire or explosion.
－ Do not pick up flammable materials or reactive metals.
－ Battery release hydrogen. Keep away from sparks or open fire.

Battery compartment shall be kept open while charging .
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Warning: Risk of electric shock. Before maintancing the machine, pls disconnect the battery cable.
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Warning: When the rotating brush running, do not touch it. Turn off the power before servicing the machine.
The following situation would be dangerous to the operator or equipment :

For security purposes

1. Do not operate the machine：

－ Contact with flammable liquids or near flammable gases,

  It could cause an explosion or flash fire situation.

－ Unless you have been trained and authorized to operate the machine.

－ Unless you have read and understood the Operator's Manual

－ If not in the case of correct operation.

2. Before starting the machine：

－Make sure that all safety devices are on positioning and operating properly.

3. When using the machine：

－ Go slow on inclines and slippery surfaces.

－ Wearing non-slip shoes.

－ Please slow down when turning.

－ When the Machinery Breakdown or faulty operation pls immediately report.

－ Do not let children play on or near the machine.

－ Follow mixing and handling instructions on chemical containers.

4. Before leaving and maintancing the machine ：

－ Park the machine on a stable surface.

－ Turn off the machine.

5. When maintancing the machine：

－ Avoid to move the accessories. Do not wear loose T-shirt, shirt or cuff.

－Before operating the machine, disconnect the battery cable.

－ Wearing protective gloves and eye protection when handling batteries or battery cable.

－ Avoid contact with battery acid fluid.

－ Do not high pressure spraying or hosed this machine.

－ Use manufacturer supplied or approved replacement parts.

－ All repairs must be performed by qualified Maintenance staff.
－ Do not modify the original design of the machine.

6. When moving the machine：

－ Pls turn off the machine.
－ Do not carry the machine when equipped with batteries.

－ Pls handle the machine with others assistance.
－ When unloading machine from a truck or trailer, use the recommended loading floor.－ Use the rope to fix the machine on a truck or trailer.

－ Put the brush head down to the lowered position.

Machine operating instructions
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Machine Installation

Open packaging machines

1.Pls check carefully to confirm that if there is a case of damage on the machine box.

If it is damaged pls response to us immediately. 

2. Check the cargo contents list ,if any missing items, please contact us.

Freight contents：

● 12V Two batteries-Standard

● 24V Charger－Standard

● A set of Battery cable - Standard

● One Squeegee blade - Standard

● One brush －Standard

● One needle plate－Standard

● Other accessories - Optional

3 Before disassemble the packing of machine , pls remove the machine fixed shipping fixture and rope on the warehouses. With assistance,unloading the machine carefully from the warehouse.

Note: If you do not use the loading floor, do not directly promote the machine to avoid Machinery Breakdown.

Note: To avoid machine damage, please unload the machine from the warehouse and then install the battery.

Install battery
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WARNING: Fire or explosion hazard. Battery release hydrogen. Keep away from sparks or open fire. The battery cover shall be kept open while charging .

1  Park the machine on level ground, and take out the key.

2  Lift the water tank so that the battery compartment is exposed can be touched.

Carefully install batteries in the battery compartment gates, and in accordance with the shown below
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          Red
Connect the battery positive cable machine

Note: Do not throwing the battery to the battery compartment, to prevent damage to the battery and the machine.

4 Before connect the battery, make sure whether the electrodes and electrical terminals are clean. As required using an electrode cleaning fluid and a wire brush.

Description: Apply in a thin layer of metal-free lubricant or spray protection on the wiring connections to avoid battery corrosion.

5. After installing the battery, pls check the power scale of battery gauge. Depending on the battery needs to charge.
Working methods of Machine

Manual control valve to adjust the amount of water on the ground through adjusting the cleaning solution (water and detergent). Brush use the mixed detergent and water solution to clean the floor . While the machine forward ,the squeegee suck the sewage into sewage tank .
Information of Brush and scouring pad

To ensure the best performance,Please use the correct brush type for cleaning.We recommend the use of brushes and scouring pads as follows:
Soft nylon brush (white)－

Recommendations for cleaning coating ground floor without injury. Clean without leaving scratches.
Polishing Pad (White)－
For maintaining a high degree of light slip or polishing the floor.
crash pad（Red）－

It used to wipe dirt slight ground without injury
Gravity folded pads（Black）－

 Removing the thick coating or substrate forcefully or scrubbing strongly 

Machine installation
1. Park the machine on level ground and remove the key.
2. The squeegee lift lever down to a lower position.
3.The vacuum suction pipe connected to the squeegee assembly.
Check the squeegee blades and make appropriate adjustments.
Brush / scouring pad Installation

Description: It is recommended to use brushes and scouring pads, refer to the manual "Brush and scouring pad Information" one.
Park the machine on level ground and remove the key.
2. Slam brush lift pedal，so that the brush head is raised off the ground.
3. First scouring pad is set with the needle seat, and then install the driver disk.Tighten the central lock will be fixed scouring pad.
Insert the needle/brush installed column bolt on motor drive tray card clasp, press the brush plate of the motor switch.

To dismount the hub and brush, brush lift pedal slam, so the head is raised off the ground, press the brush motor switch plate.

Machine operation

FOR SAFETY: Before operating manual has not been read and understood. Do not operate the machine.
WARNING: Fire or explosion hazard. Do not located near or flammable liquids, gases or combustible dust place to operate the machine

Preflight Checks

□Clean the dust on the ground.

□Check battery power scale gauge. (Refer to the battery charge gauge)

□Check the wear condition of scouring pad / brush.

□Check the wear condition of squeegee blade, and adjust the angle.
□Determine the recovery tank is empty,and clean floating filter has been installed.
□Check the wear condition of brush.

Operating machine

1. Key to turn on the main power supply to (I) position.
2. The squeegee lift lever to pull down, so that the squeegee assembly lowered to the ground.

3. On the brush head lifting pedal, make the brush head fell to the ground.
Open the water control knob.
Press the brush plate motor switch, then press the suction motor switch.

Motor drive models: The speed control knob to your desired cleaning speed

Note: We recommend the use of 45-60 meters per minute cleaning speed.

During operation of the machine

WARNING: Fire or explosion hazard. Do not pick up flammable materials or reactive metals.
Each channel overlap 5 cm cleaning path.
The machine continues to avoid damage to the ground.

3. Such as squeegee absorbing water, the ground drag marks, wipe with a cloth tape to remove garbage. Prior produce clean to prevent drag marks.
4. Do to the slope exceeds 5% (3 °) slope to operate the machine.
FOR SAFETY: When using machine, on slopes and slippery surface of the ground, move slowly.

5. If too much foam, will recommend the use of anti-foaming agent solution was poured into water tank.
Note: Do not allow foam to enter the filter, in order to avoid damage to the vacuum motor. Foam will filter switch does not fail.

6. Use double cleaning method to clean heavily soiled areas. First squeegee lifted for cleaning, let the impregnation solution 3-5 minutes, will lower the squeegee and clean again.7. Depending on the need to replace or rotate scouring pad.
8. Observe the battery power consumption table (refer "Battery power table").

9.check the remaining amount of liquid through water tank level gauge.Traditional laundry way: water consumption is 10L per 10 minutes.

10. When the water in box runs out, empty the water tank firstly and then re-inject the solution.

11.When staff leave the machine, place the machine parked on level ground and remove the key.

12. After cleaning, carry out daily maintenance procedures (see "Machine Maintenance").

Battery charge gauge

Battery charge gauge displays the battery's power. When the batteries are fully charged, all the lights are on. With power consumption, the light will go out from right to left. To prolong battery life, do not let the light goes out less than the following electricity consumption.

Note: To extend battery life, be sure to use the machine total number of more than 30 minutes before the battery be charged.

Tank Drain

After using, the recovery of tank should be drained and cleaned. The tank should be cleaned regularly to remove any corroded areas. Handling the machine to the drainage location, turn off the power key, Drainage discharge follow instructions: 

FOR SAFETY: Before leaving or servicing machine, stop on level surface and turn off machine and remove key. 

According to the counterclockwise direction to unscrew the recovery tank drain cover, remove it.

Open the cover of tank and flush it.

Remove and rinse bits floating in the sewage tank filter.

 Battery charge

Note: To prolong battery life and ensure the best performance of the machine, the machine must be used more than 30 minutes to carry out the battery charge. Do not let the battery on a state of no power for long time. The following charging instructions are applicable to this machine comes with a charger. Be sure to use the following specifications of the charger, so as not to damage the battery. 

Battery charger:

●Charger type: - Lead-acid battery charger

●Output voltage: - 24 V

●Output electric current: - 15Am

●Automatic power-off circuit


●Suitable for deep cycle type battery charge

1. Moving the machine to a well-ventilated place for charging.
WARNING: Fire or explosion hazard. Battery release hydrogen. Keep away from sparks or open fire. Shall be kept open while charging the battery compartment.

Park the machine on level ground, and turn key to the off position.

Before charging, check the electrolyte level in the battery unit

FOR SAFETY: When servicing machine, wear protective gloves and eye protection when handling batteries and battery connections. Avoid contact with battery acid fluid.

When charging, opening the side of water tank for ventilation.

The charger AC (alternating current) power cord into a properly grounded electrical outlet.

The charger's DC (direct current) cable into the rear of the recovery tank battery charging socket.

The charger will charging automatically and shut down automatically when they are filled.

Explanation: The machine will not operate when connected to the charger. Note: During charger, do not pull the charger DC line

Pull the socket out of the machine. In order to avoid arcing. Such as charging way must suspend charging Unplug the AC power cord.

WARNING: Fire or explosion hazard. Battery release hydrogen. Keep away from sparks or open fire. Shall be kept open while charging the battery compartment.

After charging, check the electrolyte surface height again.

Machine Maintenance

If you follow the maintenance procedures every day, every week and every month. the machine can be kept in the best working performance. Warning: Risk of electric shock. Before performing any maintenance disconnect the battery cable.

Daily maintenance (after each using)

1. Drain and clean the recovery tank

2. Detaching and rinse water tank located floating filter

3. Drain water tank, and depending on the need, Rinse the tank by less 60 ℃ hot water.

4. Unloading take scouring pad / brush to clean. If worn, flip or replace scouring pad

5. Wipe the squeegee blade. The squeegee assembly placed in the raised position to prevent tape damage.

6. Check the wear condition of the squeegee blade edge of the strip. Subject to wear and tear, the strip two swap.

7. Multipurpose cleaner and a damp cloth to wipe the machine. FOR SAFETY: When cleaning up the machine, do not spray or high pressure water pipe flushing machines. In order to avoid failure of electronic components.

8. Check the wear condition of the head skirt, replace if loss or damage verdict.

9. Battery charge. In order to prolong battery life and ensure the best performance of the machine, you must use the time over in the machine over 30 minutes or more to carry out the battery charge.

Monthly maintenance (after using 80 hours)

Removing the water tank and filter from the machine, then clean the filter. Make sure empty the water tank before removing the filter.

Clean the top surface of battery to avoid electrode corrosion (see "Battery Maintenance").

Check the battery wiring is loose or not.

4.Check and clean the seal of the recovery tank cover. If damaged please replaced it
5.Spray the silicone dry lubricant on all pivots and wheels.Then covered with a layer of waterproof lubricant oil, in order to maintain the smooth operation of the axle.
6.Check if the nuts and bolts on the machine are loose
7.Check if the machine leaks out
Quarterly Maintenance

Check the wear of drive motor (drive models), vacuum motor and brushes
and motor brush every 250 hours.When the length of the carbon brush wear within 10 mm, the need for carbon brush. It needs to replace the carbon brush. [image: image25.jpg]


[image: image10]If the machine need to repair, please please contact the authorized service center.
Warning:Electric Shock Risk.Please disconnect the battery wire before the maintenance machine.

Handling Machine

When using the truck or trailer moving the machine, please be sure to follow these bundled programs:

1. Raise the head to transport position.
2. Use the recommended loading floor to load machine.
3.The front of the machine adjoins to the front part of the truck or trailer. After the machine is put in place, lowing the head of brush and turning the key to the closed position.

4. Place obstacles in the rear of each drive wheel to prevent the machine slides.

5.Use the rope to fix the top of machine in order to prevent slanting.You must furnish the brackets in the truck or trailer’s car plates. For security reason:

When moving the machine, use loading floor to load machine from the truck or trailer,and rope the machine to fix the car plate.
The Storage Of Machine

Please charge the battery before storage. Do not store when the battery is flat.

2. Drain and rinse clean the flume box completely .
3. Please store the machine in a dry place, and the brush head should be kept in the rising position.

4. Open the sewage tank cover for ventilation. Note: Do not allow the machine to rain, please store in the interior.

5. If store the machine in the cold environment, please drain all the liquid inside the machine.
Operational steps
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MACHINE COMPONENTS
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	Serial number
	Part number
	
	Name
	Qty

	1
	SJ53001
	底座架组件530


	Base frame assembly 530
	1

	2
	SJ53002
	扒头支架组件530 


	Grill head support assembly
	1

	3
	SJ53003
	刷盘组件530


	Brush disc assembly
	1

	4
	SJ53004
	水路


	waterway
	1

	5
	SJ53005
	污水箱


	bilge tank
	1

	6
	SJ53006
	清水箱530 


	Clean water tank
	1

	7
	SJ53007
	扒头组件


	Raking head assembly
	1


1.Base frame assembly 530
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	序号
	零件代号
	名称
	Name
	Qty

	1
	A010105
	底座架
	Aase frame
	1

	2
	A010108
	机头提升支架
	Machine head lift bracket
	1

	3
	A010123
	轮轴限位板
	Axle limit plate
	2

	4
	A010122
	轮轴固定板
	Axle fixing plate
	2

	5
	C010100
	脚轮连接轴
	Caster connecting shaft
	1

	6
	G010130
	外六角M8×20
	Outer hexagon M8×20
	18

	7
	G010150
	外六角M8×35
	Outer hexagon M8×35
	2

	8
	G010140
	外六角M8×30
	Outer hexagon M8×30
	3

	9
	G010103
	弹垫M8
	Spring pad M8
	10

	10
	G010104
	平垫圈M8X16X1.5
	Flat washer M8X16X1.5
	22

	11
	G010108
	自锁螺母M8
	Self-locking nut M8
	13

	12
	G010166
	自锁螺母M12
	Self-locking nut M12
	2

	13
	G010110
	自锁螺母M6
	Self-locking nut M6
	2

	14
	G010131
	驱动脚轮Φ200X50
	Bearing caster Φ200X50
	2

	15
	G010165
	3寸万向轮
	3 inch universal wheel
	2

	16
	A010111
	踏板支架
	Pedal bracket
	1

	17
	A010112
	过滤器支架
	Filter holder
	1

	18
	C010108
	铜套Φ8xΦ12x17
	Copper sleeve Φ8xΦ12x17
	2

	19
	G010138
	平垫圈M8x24×2
	Flat washer M8x24×2
	6

	20
	G010106
	内六角沉头M6×20
	Hexagon countersunk head M6×20
	2


2.Grill head support assembly
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	Serial number
	Part number
	
	Name
	Qty

	1
	C010101
	吸扒连接轴
	Suction connecting shaft
	1

	2
	G010139
	外卡环φ9
	Outer snap ring φ9
	2

	3
	A010101
	扒头上支架
	top bracket
	1

	4
	A010102
	扒头下支架
	Bottom bracket
	1

	5
	G010140
	外六角M8×30
	Outer hexagon M8×30
	2

	6
	G010108
	自锁螺母M8
	Self-locking nut M8
	2

	7
	C010109
	铜套Φ8xΦ12x9
	Copper sleeve Φ8xΦ12x9
	2

	8
	G010141
	尼龙垫片12x24x2
	Nylon Spacer 12x24x2
	4

	9
	G010138
	平垫圈M8x24×2
	Flat washer M8x24×2
	2

	10
	C010114
	拉簧Φ2.8XΦ20X109
	Tension spring Φ2.8XΦ20X109
	1

	11
	C010112
	扒头拉线
	Pull the head
	1


3.Brush disc assembly
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	序号
	零件代号
	名称
	Name
	

	1
	C010119
	刷盘罩530
	Brush cover 530
	1

	2
	A010110
	机头支架
	head support
	1

	3
	A010109
	机头支架
	head support
	1

	4
	C010120
	磁吸刷盘扣
	Magnetic brush disc buckle
	1

	5
	B010117
	19寸刷盘
	19 inch brush plate
	1

	6
	G010138
	平垫圈M8x24×2
	Flat washer M8x24×2
	3

	7
	B010113
	机头防撞轮Φ100x20
	Machine head anti-collision wheelΦ100x20
	1

	8
	G010111
	外六角半牙M8×50
	Hexagonal half tooth M8×50
	1

	9
	G010140
	外六角M8×30
	Outer hexagon M8×30
	4

	10
	G010130
	外六角M8×20
	Outer hexagon M8×20
	1

	11
	G010141
	尼龙垫片12x24x2
	Nylon Spacer 12x24x2
	1

	12
	A010104
	磁吸刷盘片
	Magnetic brush disc
	1

	13
	G010104
	平垫圈M8X16X1.5
	Flat washer M8X16X1.5
	6

	14
	G010137
	平垫φ6x12x1
	Flat pad φ6x12x1
	4

	15
	G010120
	平垫φ5x10x1
	Flat pad φ5x10x1
	2

	16
	G010103
	弹垫M8
	Spring pad M8
	5

	17
	G010126
	弹垫M6
	Spring pad M6
	4

	18
	G010121
	弹垫M5
	Spring pad M5
	2

	19
	G010106
	内六角圆柱头螺钉M6×20
	Hexagon socket head screw M6×20
	4

	20
	G010134
	内六角圆柱头螺钉M5×16
	Hexagon socket head screw M5×16
	2

	21
	E010113
	刷盘电机 24V 550W Φ18
	Brush motor 24V 550W Φ18
	1

	22
	C010108
	铜套Φ8xΦ12x17
	Copper sleeve Φ8xΦ12x17
	1

	23
	C010109
	铜套Φ8xΦ12x9
	Copper sleeve Φ8xΦ12x9
	3

	24
	G010164
	内六角沉头螺钉M5×16
	Hexagon socket head countersunk head screw M5×16
	6

	25
	G010135
	自锁螺母M5
	Self-locking nut M5
	4

	26
	G010100
	十字槽盘头螺钉M5×12
	Cross recessed pan head screw M5×12
	2

	27
	A010106
	电磁阀支架
	Solenoid valve bracket
	1

	28
	E010103
	电磁阀 24V
	Solenoid valve 24V
	1

	29
	B010118
	裙边530
	skirt 530
	1

	30
	G010108
	自锁螺母M8
	Self-locking nut M8
	1

	31
	G010163
	深沟球轴承6001
	Deep groove ball bearing 6001
	2

	32
	G010150
	外六角M8×35
	Outer hexagon M8×35
	1


5.Bilge tank
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	序号
	零点代号
	名称
	Name
	

	1
	A010114
	吸水电机盖板
	Suction motor cover
	1

	2
	B010107
	排污管 Φ38*600（01+09）
	Sewage pipe Φ38*600 (01+09)
	1

	3
	B010106
	吸污管Φ38x1100（01+0 7）
	Sewage suction pipe Φ38x1100 (01+0 7)
	1

	4
	B010101
	污水箱530
	Wastewater tank 530
	1

	5
	B010102
	污水箱盖530
	Recovery tank cover 530
	1

	6
	A010115
	污水箱盖连接件
	Recovery tank cover connector
	2

	7
	G010167
	内六角圆柱头螺钉M5×20
	Hexagon socket head screw M5×20
	4

	8
	G010106
	内六角圆柱头螺钉M6×20
	Hexagon socket head screw M6×20
	2

	9
	G010162
	内六角圆柱头螺钉M6×85
	Hexagon socket head screw M6×85
	3

	10
	G010121
	弹垫M5
	Spring pad M5
	9

	11
	G010126
	弹垫M6
	Spring pad M6
	5

	12
	G010120
	平垫φ5x10x1
	Flat pad φ5x10x1
	2

	13
	G010138
	平垫圈M8x24×2
	Flat washer M8x24×2
	2

	14
	G010124
	大垫圈5x15x1.5
	Large washer 5x15x1.5
	5

	15
	G010118
	平垫圈M6x18×1.5
	Flat washer M6x18×1.5
	3

	16
	G010158
	六角螺母M8
	Hex Nut M8
	1

	17
	G010132
	外六角M8×25
	Outer hexagon M8×25
	1

	18
	G010100
	十字槽盘头螺钉M5×12
	Cross recessed pan head screw M5×12
	5

	19
	G010127
	卡箍33-57
	Clamp 33-57
	1

	20
	G010125
	水箱盖密封条
	Water tank cover seal
	1

	21
	E010114
	吸水电机 24V 500W（旁管）
	Water suction motor 24V 500W (bypass)
	1

	22
	G010119
	电机密封圈Φ150xΦ105x 13
	Motor sealing ring Φ150xΦ105x 13
	1

	23
	G010161
	PU棒
	PU stick
	3

	24
	B010111
	吸污口主体
	Main body of suction port
	1

	25
	G010123
	吸污口密封垫
	Suction port gasket
	1

	26
	G010122
	吸污口滤网
	Suction filter
	1


 6.Clean water tank
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	Serial number
	Part number
	
	Name
	Qty

	1
	B010100
	清水箱530
	Clear water tank 530
	1

	2
	B010104
	电机罩530
	Motor cover 530
	1

	3
	G010105
	合页65x65
	Hinge 65x65
	2

	4
	G010107
	胶木手柄M8X40
	Bakelite handle M8X40
	2

	5
	G010117
	内六角圆柱头螺钉M6×16
	Hexagon socket head screw M6×16
	5

	6
	G010153
	内六角圆柱头螺钉M8x20
	Hexagon socket head screw M8x20
	8

	7
	G010126
	弹垫M6
	Spring pad M6
	4

	8
	G010103
	弹垫M8
	Spring pad M8
	15

	9
	G010137
	平垫φ6x12x1
	Flat pad φ6x12x1
	4

	10
	G010104
	平垫圈M8X16X1.5
	Flat washer M8X16X1.5
	10

	11
	G010120
	平垫φ5x10x1
	Flat pad φ5x10x1
	6

	12
	G010108
	自锁螺母M8
	Self-locking nut M8
	4

	13
	G010152
	自锁螺母M3
	Self-locking nut M3
	6

	14
	G010110
	自锁螺母M6
	Self-locking nut M6
	2

	15
	G010135
	自锁螺母M5
	Self-locking nut M5
	1

	16
	G010138
	平垫圈M8x24×2
	Flat washer M8x24×2
	8

	17
	G010140
	外六角M8×30
	Outer hexagon M8×30
	1

	18
	G010154
	外六角M6×25
	Outer hexagon M6×25
	1

	19
	G010151
	外六角M3×20
	Outer hexagon M3×20
	6

	20
	G010155
	外六角M8×45
	Outer hexagon M8×45
	2

	21
	G010132
	外六角M8×25
	Outer hexagon M8×25
	5

	22
	G010106
	内六角沉头M6×20
	Hexagon countersunk head M6×20
	8

	23
	G010101
	塑料平垫M5
	Plastic flat pad M5
	8

	24
	G010109
	六角螺母M6
	Hex Nut M6
	1

	25
	G010158
	六角螺母M8
	Hex Nut M8
	1

	26
	G010116
	十字槽盘头自攻螺钉ST4. 2×13
	Cross recessed pan head tapping screw ST4. 2×13
	6

	27
	G010156
	过滤网
	Filter
	1

	28
	G010157
	链条
	chain
	1

	29
	G010160
	扎带固定座
	cable tie holder
	3

	30
	G010100
	十字槽盘头螺钉M5×12
	Cross recessed pan head screw M5×12
	17

	31
	A010103
	扒头提升摇臂
	Lifting rocker arm
	1

	32
	E010106
	过载保护器 25A
	Overload protector 25A
	1

	33
	E010105
	过载保护器45A
	Overload protector 45A
	1

	34
	A010124
	开关面板
	switch panel
	1

	35
	E010112
	钥匙开关
	key switch
	1

	36
	A010116
	摇臂支架
	rocker bracket
	1

	37
	B010103
	手柄530
	handle 530
	1

	38
	A010117
	压力支架
	pressure bracket
	1

	39
	A010119
	压力支架摇臂
	Pressure bracket rocker arm
	1

	40
	A010130
	操纵杆
	joystick
	1

	41
	E010118
	调速旋钮
	Speed ​​knob
	1

	42
	A010129
	控制面板
	control panel
	1

	43
	A010121
	排污管挂钩
	Sewage pipe hook
	1

	44
	A010113
	清水箱支架
	Fresh water tank bracket
	1

	45
	A010107
	机头清水箱支架
	Machine head clean water tank bracket
	1

	46
	A010120
	注水口钣金
	Sheet metal of water injection port
	1

	47
	C010110
	铜套Φ8XΦ12X4
	Copper sleeve Φ8XΦ12X4
	1

	48
	C010111
	铜套Φ6xΦ10x6
	Copper sleeve Φ6xΦ10x6
	1

	49
	E010111
	电量显示表
	battery indicator
	1

	50
	E010110
	翘板开关
	rocker switch
	3

	51
	E010117
	前进后退开关
	forward and backward switch
	1

	52
	F010102
	控制面板标签530
	Control Panel Tab 530
	1

	53
	A010128
	微动开关支架
	Micro switch bracket
	1

	54
	E010119
	微动开关
	Micro Switch
	1

	55
	C010118
	拉簧35x16x1.2
	Tension spring 35x16x1.2
	1

	56
	F010103
	开关面板标签530
	Switch Panel Label 530
	1

	57
	A010118
	压力支架连杆
	pressure bracket link
	2

	58
	C010115
	拉簧Φ3xΦ25x170
	Tension spring Φ3xΦ25x170
	1

	59
	F010104
	加压标签
	Pressurized labels
	1

	60
	C010103
	铜套 Φ8xΦ12x8/Φ16x2
	Copper sleeve Φ8xΦ12x8/Φ16x2
	1

	61
	C010113
	压簧Φ3XΦ17X22
	Compression spring Φ3XΦ17X22
	1

	62
	C010114
	拉簧Φ2.8XΦ20X109
	Tension spring Φ2.8XΦ20X109
	1

	63
	B010115
	加水口盖530
	Water filler cap 530
	1

	64
	B010116
	小加水口盖
	Small water filler cap
	1

	65
	C010105
	水箱拉线350
	Water tank cable 350
	1

	66
	E010122
	安德森插头50A
	Anderson plug 50A
	1

	67
	E010121
	电池24V100Ah
	Battery 24V100Ah
	1

	68
	E010120
	大灯530
	Headlight 530
	1

	69
	G010115
	橡胶密封塞
	Rubber sealing plug
	2

	70
	G010114
	塑料弯头
	plastic elbow
	2

	71
	G010159
	液位显示管φ10xφ13
	Liquid level display tube φ10xφ13
	1


7.Suction raking system
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	Serial number
	No.
	中文品名
	Name
	Quantity

	1
	SJ530007001
	防撞轮
	Anti-collision wheel
	2

	2
	SJ53007002
	吸耙主机架
	Suction rake main frame
	1

	3
	SJ53007003
	吸耙支架
	Suction harrow support
	2

	4
	SJ53007004
	压条
	Iron accessories
	1

	5
	SJ53007005
	前吸水橡胶条
	Front absorbent rubber
	1

	6
	SJ53007006
	后压条
	Water absorbent rubber layering
	1

	7
	SJ53007007
	后吸水橡胶条
	Rear water absorption rubber
	1

	8
	SJ53007008
	压条
	Absorb water Rubber sheet Iron sheets
	1

	9
	SJ53007009
	螺栓
	Screw
	4

	10
	SJ53007010
	十字螺母
	Cross nut
	4
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Trouble excluding

	Problem 
	Reason 
	Solution

	The machine can not operate
	Battery no power
	Charging the batteries

	
	Battery Fault
	Replacing the battery

	
	Loose battery cable
	Tighten the battery cable

	
	Main fuse blown
	Replace the fuse

	Brush motor does not work
	Brush lifted off the ground
	Lower brush

	
	Battery charge gauge locked does not start
	Charging the batteries

	
	Brush motor Circuit breaker tripped
	Reset the button of brush circuit breaker 

	
	Brushes (up / down) switch failure
	Please contact the service center

	
	Motor carbon brush fray
	Please contact the service center

	Vacuum motor does not work
	The squeegee is raised off the ground
	Lower squeegee

	
	Vacuum motor fuse has blown
	Replace the fuse

	
	Vacuum motor or wiring fault
	Please contact the service center

	
	Motor carbon brush fray
	Please contact the service center

	Small or anhydrous outflow
	Solution tank filter or solution tube blockage
	Cleaning solution tank filter

	
	The flow rate of the flow control knob is set too low
	Adjust the water flow control knob

	
	Release control knob screw
	After lubricating the knob locking screw

	Low recovery efficiency of sewage
	Sewage tank is full
	Drain the recovery tank

	
	Squeegee blade fray
	Replace the squeegee blade

	
	Suction tube blockage
	Clear clogged debris

	
	Sewage tank seal damage
	Replace sealing strip

	
	Vacuum motor failure
	Please contact the service center

	Running time shortened
	Battery defective
	Replace battery

	
	Battery charge fault
	Repair or replace battery charger


Hand Push Floor Scrubber

	Technical Specification
	 UNIT
	SJ700D

	Voltage
	V/AH
	24/120

	Brush motor
	W
	300*2

	 Sucker motor
	W
	500

	Driven motor 
	W
	300

	Cleaning width
	mm
	660

	Suction width
	mm
	780

	Cleaning efficiency
	m2/h
	3100

	Brushing rotation speed
	Rpm
	185

	Sucking power
	Mbar
	180

	Clean water tank capacity
	L
	50

	Sewage tank capacity
	L
	56

	Machine weight (with battery)
	Kg
	240

	Length ×width ×height
	Cm
	136*58*126


MACHINE DIMENSIONS
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